{"DATABASE":  [
{
"PROCESSOR_MODEL_NAME": "A10-6700T",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD670TYHA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-9370",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4700 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.912 V",
"PROCESSOR_TDP": "220 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD9370FHHKWOF",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-9590",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 5000 MHz",
"PROCESSOR_MULTIPLIER": "23.5x",
"PROCESSOR_VOLTAGE": "1.912 V",
"PROCESSOR_TDP": "220 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD9590FHHKWOF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6800K",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "4100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4400 MHz",
"PROCESSOR_MULTIPLIER": "41.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD680KWOA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8670D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6700",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6700OKA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8670D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-6600K",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "39.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD660KWOA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8570D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-6500",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6500OKA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8570D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-6400K",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "39.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD640KOKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8470D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-6300",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6300OKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8370D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-4000",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD4000OKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD6350FRW6KHK",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4350FRW4KHK",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 280",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX280OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4130",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4130WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-2000",
"PROCESSOR_SOCKET_IMAGE": "201.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1750 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM2000GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7340",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E1-1500",
"PROCESSOR_SOCKET_IMAGE": "42.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1480 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1500GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8350FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8300FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8140",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8140WMW8KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8170",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4500 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6120WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6130",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6130WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4120WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4150",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4150WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD6300WMHKBOX",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4320",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8320",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8320FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4300WMW4MHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5800K",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "38.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD580KWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5600K",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD560KWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5700",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5700OKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-5400K",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD540KOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7540D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5500",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5500OKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5800B",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "38.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD580BWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5500B",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD550BOKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-5400B",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD540BOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7540D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-5300B",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD530BOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-5300",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5300OKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E1-1200",
"PROCESSOR_SOCKET_IMAGE": "42.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1200GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-1800",
"PROCESSOR_SOCKET_IMAGE": "201.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1800GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7340",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6200",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6200FRW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4170",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4170FRW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 641",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD641XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 638",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD638XOJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3870K",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3870WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3670K",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3670WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3820",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3820OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3620",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3620OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3420",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3420OJZ22HX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 651",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD651XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 651K",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD651KWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8150",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8150FRGUBOX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8120FRGUBOX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6100WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4100WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8100WMW8KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3400",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3400OJZ22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3300",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD33000OJZ22HX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-3200",
"PROCESSOR_SOCKET_IMAGE": "40.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "ED3200OJZ22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6370D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3500",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3500OJZ33GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 631",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD631XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 130",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX130HBK12GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 650T",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD650TWFK4FGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 270",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX270OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3850",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3850WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3650",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3650WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3600",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3600OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3800",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3800OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 850",
"PROCESSOR_SOCKET_IMAGE": "186.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "HDX850WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 980 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ980FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 425e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD425EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 460",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX460WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 620e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD620EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 975 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ975FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 840",
"PROCESSOR_SOCKET_IMAGE": "186.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "HDX840WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1100T BE",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDE00ZFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1065T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT65TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 565 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ565WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 455",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX455WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 150",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX150HBK13GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 970 BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HDZ970FBK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 715 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ715WCJ3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1075T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT75TFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 560 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ560WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 210e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD210EHDK22GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 220",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX220OCK22GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 450",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX450WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 970 BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HDZ970FBK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 420e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD420EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 615e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD615EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 645",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX645WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 265",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX265OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 270u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD270USCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD250EHDK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 145",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX145HBK13GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1045T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT45TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 840T",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD840TWFK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 180",
"PROCESSOR_SOCKET_IMAGE": "199.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "SDX180HDK22GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 960T BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD96ZTWFK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 245e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD245EHDK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 260",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX260OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 415e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD415EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 445",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX445WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B97",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB97WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B77",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB77WFK3DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B57",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB57WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 610e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD610EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 640",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX640WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 570 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ570WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1055T (95W)",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT55TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1090T BE",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT90ZFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1055T (125W)",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT55TFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1035T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT35TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 910e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD910EOCK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 555 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ555WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 255",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX255OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 440",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX440WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 635",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX635WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 720",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDX720WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 965 BE (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ965FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 550",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDX550WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 400e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD400EHDK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 405e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD405EHDK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD250USCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 260u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 235e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD235EHDK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 240e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD240EHDK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 215",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX215OCK22GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 425",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX425WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 600e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD600EHDK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 605e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD605EHDK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 435",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX435WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B93",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB93WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B95",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB95WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B73",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB73WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B75",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB75WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B53",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB53WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B55",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB55WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 620",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX620WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 630",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX630WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 740 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ740WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 820",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX820WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 830",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX830WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 965 BE (140W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ965FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 240",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX240OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 245",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX245OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 945 (95W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX945WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 140",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX140HBK13GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX250OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 700e",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HD700EOCK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 705e",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HD705EOCK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 900e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD900EOCK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 905e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD905EOCK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 545",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDX545WFK2DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (per core)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 550 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ550WFK2DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II 42 TWKR Black Edition",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 925",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX925WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7850 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD785ZWCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 945 (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX945FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ955FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX955FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 (95W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX955WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 710",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDX710WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 805",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX805WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 720 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ720WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 810",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX810WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 910",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX910WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 920",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX920XCJ4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 940 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ940XCJ4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2650e",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADG2650IAV4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7450",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD7450WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7550",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD7550WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7750 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD775ZWCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 5050e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH5050IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8850",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8850WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9450e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9450ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 (95W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9850WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9950 BE (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD995ZXAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8250e",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8250ODJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8450e",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8450ODJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8750 BE",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD875ZWCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 6500 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD6500WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD975BWCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD985BWCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9150e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9150ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9350e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9350ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9850XAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2000+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADF2000IAV4DR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1660",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1660IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD960BWCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8450",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8450WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8650",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8650WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8750",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8750WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8550",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8550WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4050e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4050IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4450e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4450IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADA5800IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1640",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1640IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9100e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9100OBJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9550",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9550WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9650",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9650WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750 (95W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9750WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750 (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9750XAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 BE",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD985ZXAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9950 BE (140W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD995ZFAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8400",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8400WCJ3BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8600",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8600WCJ3BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4850e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4850IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2100",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2100IAA4DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2200",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2200IAA4DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2300",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2300IAA4DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2100",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2100IAA4DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+ BE",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2600+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADG2600IAV4DR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600 BE",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD960ZWCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9500",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9500WCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9600WCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5200IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2300",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2300IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2350",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2350IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2400",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1250",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1250IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1300",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1300IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1600",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADH1600IAA5DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1620",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADH1620IAA5DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1640",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1640IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ BE",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6400+ BE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADX6400IAA6CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADV6000IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1100",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1100IAA3DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1150",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1150IAA3DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1200",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+ EE",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADD3500IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADV6000IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO5000IAA5CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO3600IAA5DL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-70",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX70GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-72",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX72GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-74",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX74GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-76",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX76GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3800IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA5200IAA6CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5200IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO5000IAA5CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3600+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO3600IAA4CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-62",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "243 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX62IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4800IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.075 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADD3800IAT5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4600IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4400IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4200IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4000IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3200IAA2CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3600+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3600IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3200IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-60",
"PROCESSOR_SOCKET_IMAGE": "176.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "199 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Toledo",
"PROCESSOR_PART": "ADAFX60DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 1500+",
"PROCESSOR_SOCKET_IMAGE": "166.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Venice",
"PROCESSOR_PART": "ADC1500B2X4BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3200IAA2CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2500+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2500AIO3BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-57",
"PROCESSOR_SOCKET_IMAGE": "178.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "115 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "San Diego",
"PROCESSOR_PART": "ADAFX57DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-1350",
"PROCESSOR_SOCKET_IMAGE": "304.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Oct 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5750M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5750DEC44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5550M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5550DEC44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8550G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5350M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5350DEC23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8450G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5150M",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5150DEC23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8350G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5557M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5557DFE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8550G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5745M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5745SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8610G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5757M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5757DFE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5545M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5545SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8510G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5145M",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5145SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8310G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5345M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5345SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8410G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5357M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5357DFE23HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8450G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-1450",
"PROCESSOR_SOCKET_IMAGE": "297.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1400 MHz",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1450IDJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8250",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-1250",
"PROCESSOR_SOCKET_IMAGE": "296.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1250IDJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-1200",
"PROCESSOR_SOCKET_IMAGE": "296.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1200IFJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8180",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E1-2100",
"PROCESSOR_SOCKET_IMAGE": "302.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM2100ICJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E1-2500",
"PROCESSOR_SOCKET_IMAGE": "302.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM2500IBJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8240",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E2-3000",
"PROCESSOR_SOCKET_IMAGE": "303.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1650 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM3000IBJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8280",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5000",
"PROCESSOR_SOCKET_IMAGE": "304.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "AM5000IBJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8330",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5200",
"PROCESSOR_SOCKET_IMAGE": "305.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "AM5200IAJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8400",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Z-60",
"PROCESSOR_SOCKET_IMAGE": "235.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Hondo",
"PROCESSOR_PART": "XMZ60AFVB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-4355M",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1303 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4355SHE23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7400G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-4555M",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "19 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4555SHE44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7600G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-70",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1333 MHz",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC70AFPB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6290",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-4600M",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4600DEC44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-4500M",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4500DEC44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7640G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-4400M",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4400DEC23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7520G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-4655M",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4655SIE44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7620G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-4455M",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4455SHE24HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7500G",
"PROCESSOR_CACHEL1": "92 KB",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-4300M",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1303 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4300DEC23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7420G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E2-3000M",
"PROCESSOR_SOCKET_IMAGE": "40.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "EM3000DDX22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6380G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3320M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3320DDX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3330MX",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3330HLX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3420M",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3420DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3430MX",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3430HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3520M",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3520DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3550MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3550HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-450",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1650 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME450GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6320",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-300",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME300GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-60",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1333 MHz",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC60AFPB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6290",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3300M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3300DDX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3305M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3305DDX22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3310MX",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3310HLX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3400M",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3400DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3410MX",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3410HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3500M",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3500DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3510MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3510HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3530MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3530HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Z-01",
"PROCESSOR_SOCKET_IMAGE": "234.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "6 W",
"PROCESSOR_CODENAME": "Desna",
"PROCESSOR_PART": "XMZ01AFVB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-350",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME350GBB22GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-240",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME240GBB12GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-30",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC30AFPB12GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-50",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC50AFPB22GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-74",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM74DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-75",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM75DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-77",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM77DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-88",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-64",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL64DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-65",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL65DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-67",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL67DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-72",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM72DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-84",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM84DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-85",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM85DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-62",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL62DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-80",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "32 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM80DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-82",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM82DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-86",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM86DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-87",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-60",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL60DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-70",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM70DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3600+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3600IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-44",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML44BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-42",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML42BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-40",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT40BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-37",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT37BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-40",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML40BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-28",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "32 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML28BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-28",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "22 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT28BQX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "1.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "83 W",
"PROCESSOR_CODENAME": "Newark",
"PROCESSOR_PART": "AMN3400BKX5BU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3700+",
"PROCESSOR_SOCKET_IMAGE": "1.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "83 W",
"PROCESSOR_CODENAME": "Newark",
"PROCESSOR_PART": "AMN3700BKX5BU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-37",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML37BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-34",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML34BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-34",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT34BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-32",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML32BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-32",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-30",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML30BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-30",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "22 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4960X",
"PROCESSOR_SOCKET_IMAGE": "66.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AS",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4930K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4820K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4771",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1BW",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4340",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3430",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CE",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CG",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1630",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR16A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR169",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3910K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0TN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770K",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR147",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670K",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR149",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770S",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4765T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770R",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570TE",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR172",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770TE",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR183",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2010",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2130",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3210",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3335S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3970X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0WR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3225",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3350P",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2120",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2100T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G555",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G465",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR059",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G870",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR057",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR066",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0MF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "132.8 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0TA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "93.6 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3475S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR061",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2115C",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NV",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770K",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.025 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PL",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770S",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770T",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570K",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PM",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2550K",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0QH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2380P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G460",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0GR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3960X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0H9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3930K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0GW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2700K",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DG",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2130",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2125",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0AY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2120T",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR060",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2320",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G632",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR058",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G440",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1024 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-980",
"PROCESSOR_SOCKET_IMAGE": "83.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBYU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2102",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2405S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2310",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2105",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G622",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G840",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G850",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-990X",
"PROCESSOR_SOCKET_IMAGE": "50.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBVZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2390T",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR065",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2100",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2100T",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2120",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600K",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00C",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6960",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBT6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00B",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500K",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR008",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR009",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600S",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00E",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500T",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2300",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2400",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2400S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5800",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6951",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-560",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBY2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3500",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6800",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5700",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-870S",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBQ7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-970",
"PROCESSOR_SOCKET_IMAGE": "83.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBVF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-760",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBRP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-875K",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBS2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-880",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBPS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-655K",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBXL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-550",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBUD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6700",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-680",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3866 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5500",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-980X",
"PROCESSOR_SOCKET_IMAGE": "50.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBUZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-930",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3066 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBKP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3400",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6600",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-860S",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-750s",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-670",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBLT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-660",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBLV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-650",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-540",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBX7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-530",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBX7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-661",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "87 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBNE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6950",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1101",
"PROCESSOR_SOCKET_IMAGE": "100.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBMT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-960",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-870",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBJG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-860",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBJJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-750",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3200",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3300",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6500",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6500K",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGYP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-975",
"PROCESSOR_SOCKET_IMAGE": "81.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-950",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2210",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1600",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7600",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6300",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8400",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGT6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8400s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGT7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9400s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLG9U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8200s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLG9T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5400",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8300",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB5W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1500",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5300",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-965",
"PROCESSOR_SOCKET_IMAGE": "81.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-940",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-920",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2933 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7400",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGW3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8200",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB5M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 450",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SLAFZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5200",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAY7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8600",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "AT80570PJ0936M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7300",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9400",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB6B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9650",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB8W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 445",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "76 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe-CL",
"PROCESSOR_PART": "SLAGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7200",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1400",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAR2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8300",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9450",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9550",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9770",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9775",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "EU80574XL088N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9300",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4700",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0642M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2220",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1200",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8190",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAQR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8400",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8200",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2200",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9650",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAN3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4600",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0562M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 220",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "19 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SLAF2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2180",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6600 (95W)",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLACR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4400",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0412M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4500",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0492M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6850",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLAFN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6850",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "75 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6750",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6550",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA9X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2140",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA3J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2160",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 420",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 430",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 440",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6700",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLACQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6800",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6320",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1860 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA4U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6420",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA4T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9550s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGAE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6600 (105W)",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "105 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 935",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9QR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6700",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 925",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9KA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X6800",
"PROCESSOR_SOCKET_IMAGE": "12.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "75 W",
"PROCESSOR_CODENAME": "Conroe XE",
"PROCESSOR_PART": "SL9S5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6700",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6600",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6400",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6300",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9SA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4300",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SL9TB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 945",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9QQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 915",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9KB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron D 352",
"PROCESSOR_SOCKET_IMAGE": "140.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL9KM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 960",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9AP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 965 EE",
"PROCESSOR_SOCKET_IMAGE": "107.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3730 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 955",
"PROCESSOR_SOCKET_IMAGE": "107.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3460 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 950",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 940",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 930",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 920",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 631",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 641",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 651",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 661",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 672",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8Q9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 662",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8QB,",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron D 350",
"PROCESSOR_SOCKET_IMAGE": "9.gif",
"PROCESSOR_SOCKET": "Intel Socket 478",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 571",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8J7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 521",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 551",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8J5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 541",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 531",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 561",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7L9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 670",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 830",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL88SSL8CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 820",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8CP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 840",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL88RSL8CM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 820",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8CP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 840 EE",
"PROCESSOR_SOCKET_IMAGE": "108.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8FK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT EE 3.73",
"PROCESSOR_SOCKET_IMAGE": "121.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 630",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 640",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 650",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 660",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z5SL8QB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 620",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "135 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "68°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8AB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 519K",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3060 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 519K",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3060 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z3770",
"PROCESSOR_SOCKET_IMAGE": "306.gif",
"PROCESSOR_SOCKET": "Intel BGA1380",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-BGA1380",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1467 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Bay Trail-T",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "HD Graphics",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4000M",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4100E",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4102E",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4005U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4600M",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4960HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4600U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4330M",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2950M",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3550M",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4300M",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2955U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2980U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3556U",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3560Y",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2950M",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2955U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4950HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18G",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4550U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4650U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4500U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4350U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4558U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR188",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4200Y",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1900 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4200U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR170",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4250U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4258U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4288U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR189",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4010Y",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4010U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4100U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4158U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4702HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR15F",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR15E",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4750HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18J",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15H",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4702MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15J",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700EQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17L",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4930MX",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "57 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4900MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4800MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4850HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18H",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2580",
"PROCESSOR_SOCKET_IMAGE": "287.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Clovertrail",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "SGX 544MP2",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2560",
"PROCESSOR_SOCKET_IMAGE": "287.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Clovertrail",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "SGX 544MP2",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2520",
"PROCESSOR_SOCKET_IMAGE": "287.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Clovertrail",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "SGX 544MP2",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 987",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1000M",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR102",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020M",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ZY",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020E",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0VR",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1037U",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR108",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1007U",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR109",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1047UE",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10E",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 947UE",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10F",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1024 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020E",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0VR",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3439Y",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3689Y",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3339Y",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3687U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3537U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3540M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3540M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3227U",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3229Y",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3130M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3230M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3230M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3340M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3340M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3380M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3380M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3337U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3437U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2420",
"PROCESSOR_SOCKET_IMAGE": "271.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Penwell",
"PROCESSOR_PART": "SR0YF",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2480",
"PROCESSOR_SOCKET_IMAGE": "271.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Penwell",
"PROCESSOR_PART": "SR0U7",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2030M",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ZZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3525M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3365M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3632QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3632QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2760",
"PROCESSOR_SOCKET_IMAGE": "272.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Cloverview",
"PROCESSOR_PART": "SR0WW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3740QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3740QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3840QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3840QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3940XM",
"PROCESSOR_SOCKET_IMAGE": "137.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0US",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3630QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3635QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2020M",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0U1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2117U",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B980",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0J1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 997",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B830",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0HR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 887",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0VA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2328M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2377M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2117U",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2129Y",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3217UE",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120ME",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B730",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B820",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0HQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 807",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0PW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 877",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3520M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3520M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3555LE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3517U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3667U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3517UE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3110M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3110M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3217U",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3210M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3210M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3320M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3320M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3317U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3360M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3360M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3610ME",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3610ME",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3427U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B915C",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NZ",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3920XM",
"PROCESSOR_SOCKET_IMAGE": "137.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3720QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3720QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3615QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3615QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0NC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ND",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3610QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0NP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3610QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2370M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B970",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0J2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 977",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B720",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B815",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 797",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 867",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z2460",
"PROCESSOR_SOCKET_IMAGE": "271.gif",
"PROCESSOR_SOCKET": "Intel BGA 617",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Penwell",
"PROCESSOR_PART": "SR0PR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N2600",
"PROCESSOR_SOCKET_IMAGE": "56.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "uFCBGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Cedarview",
"PROCESSOR_PART": "SR0DB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N2800",
"PROCESSOR_SOCKET_IMAGE": "56.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "uFCBGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1867 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Cedarview",
"PROCESSOR_PART": "SR0DA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D2500",
"PROCESSOR_SOCKET_IMAGE": "56.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1867 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.21 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Cedarview",
"PROCESSOR_PART": "SR0D8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D2550",
"PROCESSOR_SOCKET_IMAGE": "56.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1867 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.21 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Cedarview",
"PROCESSOR_PART": "SR0VY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D2700",
"PROCESSOR_SOCKET_IMAGE": "56.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.21 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Cedarview",
"PROCESSOR_PART": "SR0D9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2670QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2675QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B960",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 967",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2350M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2430M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2430M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2367M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2760QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2760QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2860QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2860QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2960XM",
"PROCESSOR_SOCKET_IMAGE": "136.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2312M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2435M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2435M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2415M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2332M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B840",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 787",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 857",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 725C",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NX",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B940",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B950",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 957",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR089",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B710",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B800",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 847",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2557M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2467M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0D6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330E",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2357M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2340UE",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR074",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z650",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLC2Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z670",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLC2P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B810",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR088",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2312M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N570",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "87 mm²",
"PROCESSOR_PACKAGE": "uFCBGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBXE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2540M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR044",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2540M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR044",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2520M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2520M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2410M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2410M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2510E",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2515E",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR075",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2537M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR03W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310E",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR077",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6300",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBU8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium U5600",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBSM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2630QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2635QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR030",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2720QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2720QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2820QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2820QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2920XM",
"PROCESSOR_SOCKET_IMAGE": "136.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2710QE",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2715QE",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR076",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E625C",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E625CT",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E645C",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E645CT",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E665C",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E665CT",
"PROCESSOR_SOCKET_IMAGE": "269.gif",
"PROCESSOR_SOCKET": "Intel BGA1466",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Stellarton",
"PROCESSOR_PART": "SLH9H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6100",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6200",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E620",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH56",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E620T",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH5N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E640",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH55",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E640T",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH5M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E660",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH54",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E660T",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH5L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E680",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH94",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom E680T",
"PROCESSOR_SOCKET_IMAGE": "268.gif",
"PROCESSOR_SOCKET": "Intel BGA 676",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Tunnel Creek",
"PROCESSOR_PART": "SLH95",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-640M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBTN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-640M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBTN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N550",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "87 mm²",
"PROCESSOR_PACKAGE": "uFCBGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBXF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D425",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1834 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBXD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D525",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1834 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBXC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6000",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1877 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBWB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N455",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBX9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N475",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1834 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBX5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z560",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLH63",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium U5400",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z600",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z605",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLC3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z610",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z612",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z615",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z620",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z625",
"PROCESSOR_SOCKET_IMAGE": "267.gif",
"PROCESSOR_SOCKET": "Intel BGA 518",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "65 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Lincroft",
"PROCESSOR_PART": "SLBZD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N470",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1834 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBMF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D410",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBMH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4500",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGZC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-620M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2677 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBPE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-620M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2677 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBPE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom D510",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBLA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N450",
"PROCESSOR_SOCKET_IMAGE": "263.gif",
"PROCESSOR_SOCKET": "Intel BGA 559",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "123 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "6 W",
"PROCESSOR_CODENAME": "Pineview",
"PROCESSOR_PART": "SLBMG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 3150",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4400",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom CE4100",
"PROCESSOR_SOCKET_IMAGE": "270.gif",
"PROCESSOR_SOCKET": "Intel BGA 951",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Sodaville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom CE4130",
"PROCESSOR_SOCKET_IMAGE": "270.gif",
"PROCESSOR_SOCKET": "Intel BGA 951",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Sodaville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom CE4150",
"PROCESSOR_SOCKET_IMAGE": "270.gif",
"PROCESSOR_SOCKET": "Intel BGA 951",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "7 W",
"PROCESSOR_CODENAME": "Sodaville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "GMA 500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium SU4100",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGS4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium SU2700",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGS8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z515",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGMG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z550",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGPT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4300",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV SU3500",
"PROCESSOR_SOCKET_IMAGE": "138.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Penryn-L",
"PROCESSOR_PART": "SLGFM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z510P",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGPQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z510PT",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGPR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z520PT",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1334 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGPP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z530P",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLGPN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4200",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9100",
"PROCESSOR_SOCKET_IMAGE": "158.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2267 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Penryn QC",
"PROCESSOR_PART": "SLB5G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9300",
"PROCESSOR_SOCKET_IMAGE": "160.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2534 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Penryn QC XE",
"PROCESSOR_PART": "SLB5J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X9100",
"PROCESSOR_SOCKET_IMAGE": "159.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "44 W",
"PROCESSOR_CODENAME": "Penryn XE",
"PROCESSOR_PART": "SLB48",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N270",
"PROCESSOR_SOCKET_IMAGE": "262.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Diamondville",
"PROCESSOR_PART": "SLB73",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom N280",
"PROCESSOR_SOCKET_IMAGE": "262.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Diamondville",
"PROCESSOR_PART": "SLBL9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom 230",
"PROCESSOR_SOCKET_IMAGE": "262.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "25.96 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Diamondville",
"PROCESSOR_PART": "SLB6Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom 330",
"PROCESSOR_SOCKET_IMAGE": "262.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "25.96 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1625 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Diamondville",
"PROCESSOR_PART": "SLG9Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV SU3300",
"PROCESSOR_SOCKET_IMAGE": "138.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Penryn-L",
"PROCESSOR_PART": "SLGAR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z500",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "1 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLB6Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z510",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLB2C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z520",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1334 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLB2H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z530",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLB6P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Atom Z540",
"PROCESSOR_SOCKET_IMAGE": "266.gif",
"PROCESSOR_SOCKET": "Intel BGA 441",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "47 million",
"PROCESSOR_DIE_SIZE": "26 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1867 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "2 W",
"PROCESSOR_CODENAME": "Silverthorne",
"PROCESSOR_PART": "SLB2M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1073 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7800",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLAF6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7250",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA49",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV U2100",
"PROCESSOR_SOCKET_IMAGE": "139.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Merom-L",
"PROCESSOR_PART": "SLAGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV U2200",
"PROCESSOR_SOCKET_IMAGE": "139.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Merom-L",
"PROCESSOR_PART": "SLAGL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X7900",
"PROCESSOR_SOCKET_IMAGE": "154.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "44 W",
"PROCESSOR_CODENAME": "Merom XE",
"PROCESSOR_PART": "SLAF4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A100",
"PROCESSOR_SOCKET_IMAGE": "265.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stealey",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A110",
"PROCESSOR_SOCKET_IMAGE": "265.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stealey",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA44",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA43",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7100",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA4A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1073 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7600G",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket M",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9U5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo ULV L2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7200",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7400",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2166 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket M",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5200",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7300",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLAMD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2700",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo ULV L2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2250",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.31 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo ULV U1300",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo ULV U1400",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1300",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2300",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1826 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2600",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2166 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1992 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8V?",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1200",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1350",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1400",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2300",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 780",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2260 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7VB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2050",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.31 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 770",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2130 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 760",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 750",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1860 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7S9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 740",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1730 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 730",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL86G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Mobile Pentium 4 HT 552",
"PROCESSOR_SOCKET_IMAGE": "246.gif",
"PROCESSOR_SOCKET": "Intel Socket 478",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "112 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "75°C",
"PROCESSOR_FREQUENCY": "3467 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "88 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7NC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "8 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
}
]}}
