{"DATABASE": [
{
"PROCESSOR_MODEL_NAME": "Core i7-4790",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4690",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4360",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4590",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3450",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1840",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4790S",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4590S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4150T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4960X",
"PROCESSOR_SOCKET_IMAGE": "66.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AS",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4930K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4820K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4771",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1BW",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4340",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3430",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CE",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CG",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1630",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR16A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR169",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3910K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0TN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770K",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR147",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670K",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR149",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770S",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4765T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770R",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570TE",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR172",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770TE",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR183",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2010",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2130",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3210",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3335S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3970X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0WR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3225",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3350P",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2120",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2100T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G555",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G465",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR059",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G870",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR057",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR066",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0MF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "132.8 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0TA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "93.6 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3475S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR061",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2115C",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NV",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770K",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.025 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PL",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770S",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770T",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570K",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PM",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2550K",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0QH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2380P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G460",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0GR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3960X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0H9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3930K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0GW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2700K",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DG",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2130",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2125",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0AY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2120T",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR060",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2320",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G632",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR058",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G440",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1024 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-980",
"PROCESSOR_SOCKET_IMAGE": "83.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBYU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2102",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2405S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2310",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2105",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G622",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G840",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G850",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4790",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4690",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4360",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4590",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3450",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1840",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4790S",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4590S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4150T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell Refresh",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unreleased",
"PROCESSOR_RELEASED": "May 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4960X",
"PROCESSOR_SOCKET_IMAGE": "66.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AS",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4930K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4820K",
"PROCESSOR_SOCKET_IMAGE": "289.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1860 million",
"PROCESSOR_DIE_SIZE": "257 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "SR1AU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4771",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1BW",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4340",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4330T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130T",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4130",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3430",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CE",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1NB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3420T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CG",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4440S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G3220T",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1CL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1630",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR16A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR169",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3910K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0TN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770K",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR147",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670K",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4430S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR149",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770S",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4765T",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670T",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570S",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770R",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "66°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4670R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570R",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel Iris™ Pro 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4570TE",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR172",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4770TE",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR183",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2010",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2020T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2130",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3210",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0YY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1620",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1610T",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3335S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3970X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0WR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3225",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3220",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3240T",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3330S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3350P",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2120",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G2100T",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "94 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G645T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G555",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0RZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G465",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0S8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR059",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G870",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR057",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G640T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR066",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0MF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "132.8 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0TA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3470T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "93.6 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "65°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0RJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3475S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "133 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR061",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2115C",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NV",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770K",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.025 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PL",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770S",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3770T",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570K",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PM",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3550S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3570T",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3450S",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2550K",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0QH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2380P",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0G2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G460",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0GR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1536 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3960X",
"PROCESSOR_SOCKET_IMAGE": "29.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0H9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3930K",
"PROCESSOR_SOCKET_IMAGE": "135.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0GW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2700K",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DG",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2130",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2125",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0AY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2120T",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR060",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2320",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G630T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G632",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G860",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR058",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G530T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G440",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "1024 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G550T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G540T",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-980",
"PROCESSOR_SOCKET_IMAGE": "83.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBYU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2102",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2405S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2310",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2105",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G620T",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G622",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G840",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G850",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-990X",
"PROCESSOR_SOCKET_IMAGE": "50.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBVZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2390T",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR065",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2100",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2100T",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2120",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR05Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600K",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00C",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6960",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBT6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00B",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500K",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR008",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR009",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2600S",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00E",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2500T",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2300",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2400",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2400S",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5800",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6951",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-560",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBY2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3500",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6800",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5700",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-870S",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBQ7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-970",
"PROCESSOR_SOCKET_IMAGE": "83.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBVF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-760",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBRP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-875K",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBS2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-880",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBPS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-655K",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBXL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-550",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBUD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6700",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-680",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3866 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5500",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-980X",
"PROCESSOR_SOCKET_IMAGE": "50.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBUZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-930",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3066 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBKP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3400",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6600",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-860S",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-750s",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-670",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBLT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-660",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBLV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-650",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-540",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBX7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-530",
"PROCESSOR_SOCKET_IMAGE": "110.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBX7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-661",
"PROCESSOR_SOCKET_IMAGE": "15.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "87 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBNE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium G6950",
"PROCESSOR_SOCKET_IMAGE": "99.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBTG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron G1101",
"PROCESSOR_SOCKET_IMAGE": "100.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "382 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "73 W",
"PROCESSOR_CODENAME": "Clarkdale",
"PROCESSOR_PART": "SLBMT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-960",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-870",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBJG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-860",
"PROCESSOR_SOCKET_IMAGE": "84.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBJJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-750",
"PROCESSOR_SOCKET_IMAGE": "111.gif",
"PROCESSOR_SOCKET": "Intel Socket 1156",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "774 million",
"PROCESSOR_DIE_SIZE": "296 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Lynnfield",
"PROCESSOR_PART": "SLBLC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3200",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E3300",
"PROCESSOR_SOCKET_IMAGE": "102.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6500",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGUH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6500K",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGYP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-975",
"PROCESSOR_SOCKET_IMAGE": "81.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-950",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2210",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1600",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7600",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E6300",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGU9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8400",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGT6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8400s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGT7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9400s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLG9U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8200s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLG9T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5400",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGTE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8300",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB5W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1500",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5300",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-965",
"PROCESSOR_SOCKET_IMAGE": "81.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-940",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-920",
"PROCESSOR_SOCKET_IMAGE": "82.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2933 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBCH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7400",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLGW3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q8200",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB5M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 450",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SLAFZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium E5200",
"PROCESSOR_SOCKET_IMAGE": "105.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "228 million",
"PROCESSOR_DIE_SIZE": "82 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAY7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8600",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "AT80570PJ0936M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7300",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9400",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB6B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9650",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3625 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLB8W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 445",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "76 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe-CL",
"PROCESSOR_PART": "SLAGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E7200",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "420 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1400",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAR2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8300",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9450",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9550",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9770",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9775",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "EU80574XL088N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9300",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "548 million",
"PROCESSOR_DIE_SIZE": "2x 81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAWE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4700",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0642M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2220",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron E1200",
"PROCESSOR_SOCKET_IMAGE": "101.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLAQW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8190",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAQR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8400",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8200",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "104 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLAPP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E8500",
"PROCESSOR_SOCKET_IMAGE": "116.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3330 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Wolfdale",
"PROCESSOR_PART": "SLB9K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2200",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9650",
"PROCESSOR_SOCKET_IMAGE": "122.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLAN3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4600",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0562M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 220",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "19 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SLAF2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2180",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6600 (95W)",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLACR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4400",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0412M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4500",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "HH80557PG0492M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6850",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLAFN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6850",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "75 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6750",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6550",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA9X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2140",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA3J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core E2160",
"PROCESSOR_SOCKET_IMAGE": "104.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SLA8Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 420",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 430",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 440",
"PROCESSOR_SOCKET_IMAGE": "103.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.3375 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Conroe-L",
"PROCESSOR_PART": "SL9XL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6700",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SLACQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6800",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6320",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1860 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA4U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6420",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SLA4T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9550s",
"PROCESSOR_SOCKET_IMAGE": "13.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "820 million",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Yorkfield",
"PROCESSOR_PART": "SLGAE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q6600 (105W)",
"PROCESSOR_SOCKET_IMAGE": "119.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "105 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 935",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9QR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX6700",
"PROCESSOR_SOCKET_IMAGE": "123.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "582 million",
"PROCESSOR_DIE_SIZE": "2x 143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Kentsfield",
"PROCESSOR_PART": "SL9UL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 925",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9KA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X6800",
"PROCESSOR_SOCKET_IMAGE": "12.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "75 W",
"PROCESSOR_CODENAME": "Conroe XE",
"PROCESSOR_PART": "SL9S5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6700",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6600",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6400",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9S9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E6300",
"PROCESSOR_SOCKET_IMAGE": "11.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Conroe",
"PROCESSOR_PART": "SL9SA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo E4300",
"PROCESSOR_SOCKET_IMAGE": "117.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "167 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.34 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Allendale",
"PROCESSOR_PART": "SL9TB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 945",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9QQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 915",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9KB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron D 352",
"PROCESSOR_SOCKET_IMAGE": "140.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL9KM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 960",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL9AP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 965 EE",
"PROCESSOR_SOCKET_IMAGE": "107.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3730 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 955",
"PROCESSOR_SOCKET_IMAGE": "107.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3460 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 950",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 940",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 930",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 920",
"PROCESSOR_SOCKET_IMAGE": "18.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "376 million",
"PROCESSOR_DIE_SIZE": "140 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.33 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Presler",
"PROCESSOR_PART": "SL94S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 631",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 641",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 651",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 661",
"PROCESSOR_SOCKET_IMAGE": "114.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "188 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "86 W",
"PROCESSOR_CODENAME": "Cedar Mill",
"PROCESSOR_PART": "SL94V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 672",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8Q9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 662",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8QB,",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Celeron D 350",
"PROCESSOR_SOCKET_IMAGE": "9.gif",
"PROCESSOR_SOCKET": "Intel Socket 478",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 571",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8J7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 521",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 551",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8J5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 541",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 531",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 561",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7L9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 506",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 670",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 830",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL88SSL8CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 820",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8CP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 840",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL88RSL8CM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 820",
"PROCESSOR_SOCKET_IMAGE": "109.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8CP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium D 840 EE",
"PROCESSOR_SOCKET_IMAGE": "108.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "206 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Smithfield",
"PROCESSOR_PART": "SL8FK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT EE 3.73",
"PROCESSOR_SOCKET_IMAGE": "121.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 630",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 640",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 650",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 660",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7Z5SL8QB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 HT 620",
"PROCESSOR_SOCKET_IMAGE": "55.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "169 million",
"PROCESSOR_DIE_SIZE": "135 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "68°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.388 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8AB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "28 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 511",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL9CJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 519K",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3060 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 4 519K",
"PROCESSOR_SOCKET_IMAGE": "16.gif",
"PROCESSOR_SOCKET": "Intel Socket 775",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "109 mm²",
"PROCESSOR_PACKAGE": "FC-LGA4",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3060 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL8PN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2, DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4940MX",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "57 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4910MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4810MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4000M",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4100E",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4102E",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4005U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4600M",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR1H7",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4960HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR1BS",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4600U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4330M",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2950M",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3550M",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4300M",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2955U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2980U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "72°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3556U",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 3560Y",
"PROCESSOR_SOCKET_IMAGE": "311.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2950M",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 2955U",
"PROCESSOR_SOCKET_IMAGE": "276.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4850EQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR17X",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Aug 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4860EQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR195",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Aug 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4950HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18G",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4550U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4650U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4500U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16Z",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4350U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4558U",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1300 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR188",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4200Y",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1900 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4200U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR170",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4250U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4258U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-4288U",
"PROCESSOR_SOCKET_IMAGE": "308.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR189",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4010Y",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "12 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4010U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4100U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR16P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4400",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-4158U",
"PROCESSOR_SOCKET_IMAGE": "309.gif",
"PROCESSOR_SOCKET": "Intel BGA1168",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1168",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "28 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR18B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5100",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4702HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR15F",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR15E",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4750HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18J",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15H",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4702MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "37 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15J",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700EQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17L",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4700EQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR17L",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4930MX",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "57 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4900MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4800MQ",
"PROCESSOR_SOCKET_IMAGE": "310.gif",
"PROCESSOR_SOCKET": "Intel Socket G3",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "177 mm²",
"PROCESSOR_PACKAGE": "FC-PGA946",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-4850HQ",
"PROCESSOR_SOCKET_IMAGE": "291.gif",
"PROCESSOR_SOCKET": "Intel BGA1364",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "264 mm²",
"PROCESSOR_PACKAGE": "FC-BGA1364",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Crystalwell",
"PROCESSOR_PART": "SR18H",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 5200",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 987",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1000M",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR102",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020M",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ZY",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020E",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0VR",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1037U",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR108",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1007U",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR109",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1047UE",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10E",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 947UE",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR10F",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1024 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 1020E",
"PROCESSOR_SOCKET_IMAGE": "275.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0VR",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3439Y",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12Q",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3689Y",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3339Y",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "67°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3687U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3537U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3540M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3540M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3227U",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3229Y",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "13 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3130M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3230M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3230M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3340M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3340M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3380M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3380M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0X7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3337U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3437U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0XE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2030M",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ZZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3525M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3365M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3632QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3632QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3740QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3740QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3840QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3840QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3940XM",
"PROCESSOR_SOCKET_IMAGE": "137.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0US",
"PROCESSOR_PRODUCTION_STATUS": "End-of-life",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3630QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0UX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3635QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1480 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2020M",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0U1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2117U",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B980",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0J1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 997",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B830",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0HR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 887",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0VA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2328M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2377M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2117U",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 2129Y",
"PROCESSOR_SOCKET_IMAGE": "248.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR12M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3217UE",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0WN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3120ME",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B730",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B820",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0HQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 807",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0PW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 877",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3520M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3520M",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3555LE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3517U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3667U",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3517UE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0T6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3110M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3110M",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-3217U",
"PROCESSOR_SOCKET_IMAGE": "62.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3210M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3210M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3320M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3320M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3317U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3360M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3360M",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3610ME",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3610ME",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0QJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-3427U",
"PROCESSOR_SOCKET_IMAGE": "63.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0N7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B915C",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NZ",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3920XM",
"PROCESSOR_SOCKET_IMAGE": "137.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3820QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3720QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3720QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3615QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3615QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0NC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0ND",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3610QE",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0NP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3612QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-3610QM",
"PROCESSOR_SOCKET_IMAGE": "64.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-PGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0MN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2450M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2370M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B970",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0J2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 977",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B720",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B815",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 797",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 867",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2670QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2675QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B960",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 967",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2350M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2430M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2430M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2367M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2760QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2760QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2860QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2860QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2960XM",
"PROCESSOR_SOCKET_IMAGE": "136.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2312M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2435M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2435M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2415M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2332M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B840",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 787",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 857",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 725C",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0NX",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B940",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium B950",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 957",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR089",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B710",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "1536 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B800",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0EW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron 847",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR08N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2557M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2467M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR0D6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2330E",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2357M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2340UE",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR074",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Celeron B810",
"PROCESSOR_SOCKET_IMAGE": "48.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR088",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Sandy Bridge)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2312M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2540M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR044",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2540M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR044",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2520M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2520M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310M",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2410M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2410M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR04B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2510E",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2515E",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR075",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i5-2537M",
"PROCESSOR_SOCKET_IMAGE": "28.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR03W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i3-2310E",
"PROCESSOR_SOCKET_IMAGE": "14.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "624 million",
"PROCESSOR_DIE_SIZE": "149 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR077",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6300",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBU8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium U5600",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBSM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2630QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02Y",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2635QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR030",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2720QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2720QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2820QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2820QM",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1224",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2920XM",
"PROCESSOR_SOCKET_IMAGE": "136.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2710QE",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel Socket G2 (988B)",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR02T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-2715QE",
"PROCESSOR_SOCKET_IMAGE": "27.gif",
"PROCESSOR_SOCKET": "Intel BGA1023",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR076",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6100",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6200",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-640M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBTN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-640M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBTN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium P6000",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel Socket G1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1877 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBWB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium U5400",
"PROCESSOR_SOCKET_IMAGE": "249.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBUH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4500",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGZC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-620M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2677 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBPE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core i7-620M",
"PROCESSOR_SOCKET_IMAGE": "257.gif",
"PROCESSOR_SOCKET": "Intel BGA1288",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "384 million",
"PROCESSOR_DIE_SIZE": "81 mm²",
"PROCESSOR_PACKAGE": "rPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2677 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Arrandale",
"PROCESSOR_PART": "SLBPE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4400",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium SU4100",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGS4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium SU2700",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGS8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4300",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV SU3500",
"PROCESSOR_SOCKET_IMAGE": "138.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Penryn-L",
"PROCESSOR_PART": "SLGFM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium Dual-Core T4200",
"PROCESSOR_SOCKET_IMAGE": "261.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Penryn",
"PROCESSOR_PART": "SLGJN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Quad Q9100",
"PROCESSOR_SOCKET_IMAGE": "158.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2267 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Penryn QC",
"PROCESSOR_PART": "SLB5G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme QX9300",
"PROCESSOR_SOCKET_IMAGE": "160.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "2x 107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2534 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Penryn QC XE",
"PROCESSOR_PART": "SLB5J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB (per die)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X9100",
"PROCESSOR_SOCKET_IMAGE": "159.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "44 W",
"PROCESSOR_CODENAME": "Penryn XE",
"PROCESSOR_PART": "SLB48",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV SU3300",
"PROCESSOR_SOCKET_IMAGE": "138.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "107 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Penryn-L",
"PROCESSOR_PART": "SLGAR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "3072 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1073 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3V",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7800",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLAF6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7250",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA49",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV U2100",
"PROCESSOR_SOCKET_IMAGE": "139.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1067 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Merom-L",
"PROCESSOR_PART": "SLAGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Solo ULV U2200",
"PROCESSOR_SOCKET_IMAGE": "139.gif",
"PROCESSOR_SOCKET": "Intel BGA 956",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "291 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1 V",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Merom-L",
"PROCESSOR_PART": "SLAGL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Extreme X7900",
"PROCESSOR_SOCKET_IMAGE": "154.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "44 W",
"PROCESSOR_CODENAME": "Merom XE",
"PROCESSOR_PART": "SLAF4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A100",
"PROCESSOR_SOCKET_IMAGE": "265.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stealey",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A110",
"PROCESSOR_SOCKET_IMAGE": "265.gif",
"PROCESSOR_SOCKET": "Intel BGA 437",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "176 million",
"PROCESSOR_DIE_SIZE": "66 mm²",
"PROCESSOR_PACKAGE": "FC-BGA12F",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "3 W",
"PROCESSOR_CODENAME": "Stealey",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2007",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA44",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7700",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA43",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7100",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.175 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLA4A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo U7500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket P",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "111 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1073 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "0.975 V",
"PROCESSOR_TDP": "10 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLV3X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7600G",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket M",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9U5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo ULV L2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7200",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7400",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2166 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5600",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5500",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket M",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SL9SH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T5200",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core 2 Duo T7300",
"PROCESSOR_SOCKET_IMAGE": "118.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "293 million",
"PROCESSOR_DIE_SIZE": "143 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Merom",
"PROCESSOR_PART": "SLAMD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2700",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo ULV L2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2250",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.31 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo ULV U1300",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1066 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo ULV U1400",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1300",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2300",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1660 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1826 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2600",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2166 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8VN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2500",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1992 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "SL8V?",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1200",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1350",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Solo T1400",
"PROCESSOR_SOCKET_IMAGE": "67.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "76 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2300",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo LV L2400",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.212 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 780",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2260 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7VB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Core Duo T2050",
"PROCESSOR_SOCKET_IMAGE": "65.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "151 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.31 V",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Yonah",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 770",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2130 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 760",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 750",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1860 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7S9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 740",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1730 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL7SA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Pentium M 730",
"PROCESSOR_SOCKET_IMAGE": "19.gif",
"PROCESSOR_SOCKET": "Intel Socket 479",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "140 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "27 W",
"PROCESSOR_CODENAME": "Dothan",
"PROCESSOR_PART": "SL86G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "32 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Mobile Pentium 4 HT 552",
"PROCESSOR_SOCKET_IMAGE": "246.gif",
"PROCESSOR_SOCKET": "Intel Socket 478",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "125 million",
"PROCESSOR_DIE_SIZE": "112 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "75°C",
"PROCESSOR_FREQUENCY": "3467 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "88 W",
"PROCESSOR_CODENAME": "Prescott",
"PROCESSOR_PART": "SL7NC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2005",
"PROCESSOR_MEMORYSUPPORT": "DDR1, DDR2",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "8 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
}
]}}