{"DATABASE":  [
{
"PROCESSOR_MODEL_NAME": "Opteron  43CX EE",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OE43CXHPU4KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4310 EE",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4310HPU4KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4334",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4334WLU6KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4340",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4340WLU6KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4332 HE",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4332OFU6KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4386",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4386WLU8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  43GK HE",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OE43GKOHU8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  4376 HE",
"PROCESSOR_SOCKET_IMAGE": "273.gif",
"PROCESSOR_SOCKET": "AMD Socket C32",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Seoul",
"PROCESSOR_PART": "OS4376OFU8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  3320 EE",
"PROCESSOR_SOCKET_IMAGE": "288.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Delhi",
"PROCESSOR_PART": "OS3380OLW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  3350 HE",
"PROCESSOR_SOCKET_IMAGE": "288.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Delhi",
"PROCESSOR_PART": "OS3350HOW4KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron  3380",
"PROCESSOR_SOCKET_IMAGE": "288.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Delhi",
"PROCESSOR_PART": "OS3380OLW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6386 SE",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6386YETGGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6380",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6380WKTGGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6378",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6378WKTGGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6376",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6376WKTGGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6366 HE",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6366VATGGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6348",
"PROCESSOR_SOCKET_IMAGE": "247.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Abu Dhabi",
"PROCESSOR_PART": "OS6348WKTCGHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Twelve-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "576 KB",
"PROCESSOR_CACHEL2": "12288 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6284 SE",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6284YETGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6278",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6278WKTGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6262 HE",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6262VATGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB (shared)",
"PROCESSOR_CACHEL2": "8196 KB (per core)",
"PROCESSOR_CACHEL3": "16384 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6282 SE",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6282YETGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6276",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6276WKTGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB",
"PROCESSOR_CACHEL2": "16384 KB",
"PROCESSOR_CACHEL3": "8192 KB (per die)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6274",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6274WKTGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB (shared)",
"PROCESSOR_CACHEL2": "8196 KB (per core)",
"PROCESSOR_CACHEL3": "16384 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6272",
"PROCESSOR_SOCKET_IMAGE": "203.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2400 million",
"PROCESSOR_DIE_SIZE": "316 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Interlagos",
"PROCESSOR_PART": "OS6272WKTGGGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Sixteen-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB (shared)",
"PROCESSOR_CACHEL2": "8196 KB (per core)",
"PROCESSOR_CACHEL3": "16384 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 6168",
"PROCESSOR_SOCKET_IMAGE": "206.gif",
"PROCESSOR_SOCKET": "AMD Socket G34",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "1800 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "69°C",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.1875 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Magny-Cours",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Twelve-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "768 KB (shared)",
"PROCESSOR_CACHEL2": "6144 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 2350 HE",
"PROCESSOR_SOCKET_IMAGE": "211.gif",
"PROCESSOR_SOCKET": "AMD Socket Fr2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "463 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "76°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "79 W",
"PROCESSOR_CODENAME": "Barcelona",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "0",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB (shared)",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "2048 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 856",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "92 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSA856FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 185",
"PROCESSOR_SOCKET_IMAGE": "221.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Denmark",
"PROCESSOR_PART": "OSA185DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 285",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA285FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 885",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA885FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 890",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA890FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 275 HE",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSK275FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 875 HE",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 290",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA290FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 870 HE",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSK870FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 270 HE",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSK270FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 880",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA880FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 280",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA280FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 875",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA875FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 870",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA870FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 865",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSA865FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 180",
"PROCESSOR_SOCKET_IMAGE": "221.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Denmark",
"PROCESSOR_PART": "OSA180DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 175",
"PROCESSOR_SOCKET_IMAGE": "221.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Denmark",
"PROCESSOR_PART": "OSA175DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 170",
"PROCESSOR_SOCKET_IMAGE": "221.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Denmark",
"PROCESSOR_PART": "OSA170DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 165",
"PROCESSOR_SOCKET_IMAGE": "221.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Denmark",
"PROCESSOR_PART": "OSA165DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 154",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA154DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 152",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA152DAA5CF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 150",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA150DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 148",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA148DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 146",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "67 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 144",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "67 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA144DAA5CF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 152",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA152DAA5CF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 150",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA150DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 144",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "67 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA144DAA5CF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 146",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "67 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 148",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "85 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA148DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 146",
"PROCESSOR_SOCKET_IMAGE": "225.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "67 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 865 HE",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSK865FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 265 HE",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSK265FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 860 HE",
"PROCESSOR_SOCKET_IMAGE": "216.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Egypt",
"PROCESSOR_PART": "OSK860FAA6CC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 260 HE",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSK260FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 854",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "92 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSA854FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 254",
"PROCESSOR_SOCKET_IMAGE": "220.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "92 W",
"PROCESSOR_CODENAME": "Troy",
"PROCESSOR_PART": "OSA254FAA5BL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 275",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA275FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 270",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA270FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron X2 265",
"PROCESSOR_SOCKET_IMAGE": "217.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Italy",
"PROCESSOR_PART": "OSA265FAA6CB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 156",
"PROCESSOR_SOCKET_IMAGE": "224.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "Venus",
"PROCESSOR_PART": "OSA156DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 850 HE",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSK850FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 250 HE",
"PROCESSOR_SOCKET_IMAGE": "220.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Troy",
"PROCESSOR_PART": "OSK250FAA5BL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 848 HE",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSK848FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 248 HE",
"PROCESSOR_SOCKET_IMAGE": "220.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Troy",
"PROCESSOR_PART": "OSK248FAA5BL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 246 HE",
"PROCESSOR_SOCKET_IMAGE": "220.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Troy",
"PROCESSOR_PART": "OSK246FAA5BL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 846 HE",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "55 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSK846FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 852",
"PROCESSOR_SOCKET_IMAGE": "218.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "92 W",
"PROCESSOR_CODENAME": "Athens",
"PROCESSOR_PART": "OSA852FAA5BM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "8",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Opteron 252",
"PROCESSOR_SOCKET_IMAGE": "220.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "106 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "92 W",
"PROCESSOR_CODENAME": "Troy",
"PROCESSOR_PART": "OSA252FAA5BL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
}
]}}