{"DATABASE":  [
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2630L v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2609 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2643 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2630 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2620 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2637 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2603 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2640 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2650 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2667 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2687W v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2660 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2670 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2680 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2690 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2650L v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2692 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Twelve-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2695 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Twelve-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2697 v2",
"PROCESSOR_SOCKET_IMAGE": "292.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EP",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Twelve-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1620 v2",
"PROCESSOR_SOCKET_IMAGE": "294.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1650 v2",
"PROCESSOR_SOCKET_IMAGE": "294.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1660 v2",
"PROCESSOR_SOCKET_IMAGE": "294.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Ivy Bridge-E",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2403 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2407 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2420 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2430 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2440 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2450 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2470 v2",
"PROCESSOR_SOCKET_IMAGE": "293.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Ivy Bridge-EN",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "25600 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR154",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1230 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR153",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1240 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR152",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1270 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR151",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1280 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "82 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR150",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1285 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14W",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1225 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14U",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1245 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14T",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1275 v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "84 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220L v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "16 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1230L v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR158",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1265L v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR15A",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD (Haswell)",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1285L v3",
"PROCESSOR_SOCKET_IMAGE": "283.gif",
"PROCESSOR_SOCKET": "Intel Socket 1150",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Haswell",
"PROCESSOR_PART": "SR14X",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3, DDR4",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4600",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Atom S1260",
"PROCESSOR_SOCKET_IMAGE": "274.gif",
"PROCESSOR_SOCKET": "Intel BGA1283",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Centerton",
"PROCESSOR_PART": "SLK2H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "56 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Atom S1240",
"PROCESSOR_SOCKET_IMAGE": "274.gif",
"PROCESSOR_SOCKET": "Intel BGA1283",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "6 W",
"PROCESSOR_CODENAME": "Centerton",
"PROCESSOR_PART": "SLK2J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "56 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Atom S1220",
"PROCESSOR_SOCKET_IMAGE": "274.gif",
"PROCESSOR_SOCKET": "Intel BGA1283",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Centerton",
"PROCESSOR_PART": "SLK2K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "56 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1290 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "87 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1280 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1270 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1240 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1230 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "69 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1275 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1265L v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2500",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1245 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0P9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1225 v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "1400 million",
"PROCESSOR_DIE_SIZE": "160 mm²",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0PJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P4000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220L v2",
"PROCESSOR_SOCKET_IMAGE": "61.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "22 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA12C",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Ivy Bridge",
"PROCESSOR_PART": "SR0R6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4650",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0JH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4617",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0L5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4603",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0LF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4610",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0JJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4607",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0JL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4620",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0JP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "16384 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4640",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0KJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-4650L",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0JN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1410",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0RM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1428L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0JW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2403",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2407",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2418L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2100 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "50 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0M5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2420",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2430",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2440",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2428L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2000 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0JV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2430L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2450",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2470",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2448L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2100 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0JU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2450L",
"PROCESSOR_SOCKET_IMAGE": "79.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EN",
"PROCESSOR_PART": "SR0LH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1105C",
"PROCESSOR_SOCKET_IMAGE": "295.gif",
"PROCESSOR_SOCKET": "Intel BGA1283",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Gladden",
"PROCESSOR_PART": "SR0NS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1125C",
"PROCESSOR_SOCKET_IMAGE": "295.gif",
"PROCESSOR_SOCKET": "Intel BGA1283",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Gladden",
"PROCESSOR_PART": "SR0NU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2603",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0LB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2609",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0LA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2643",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0L7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2637",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0LE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "5120 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2620",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2630",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2640",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2667",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2630L",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H1",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2650",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2658",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0LZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2660",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0GZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2665",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0HB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2670",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "115 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2680",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0GY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2690",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0HA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2687W",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2650L",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0H0",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1620",
"PROCESSOR_SOCKET_IMAGE": "78.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1270 million",
"PROCESSOR_DIE_SIZE": "294 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0LC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "10240 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1650",
"PROCESSOR_SOCKET_IMAGE": "78.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0HC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-1660",
"PROCESSOR_SOCKET_IMAGE": "78.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Sandy Bridge-E",
"PROCESSOR_PART": "SR0H2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "15360 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5-2648L",
"PROCESSOR_SOCKET_IMAGE": "80.gif",
"PROCESSOR_SOCKET": "Intel Socket 2011",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2270 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Sandy Bridge-EP",
"PROCESSOR_PART": "SR0HE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "20480 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Pentium 350",
"PROCESSOR_SOCKET_IMAGE": "47.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR07S",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1290",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR055",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220L",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "504 million",
"PROCESSOR_DIE_SIZE": "131 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "20 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR070",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "3072 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1220",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1225",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "31.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00G",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1230",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00H",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1235",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00J",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1240",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00K",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1245",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00L",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1270",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1275",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00P",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD P3000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1280",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00R",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E3-1260L",
"PROCESSOR_SOCKET_IMAGE": "30.gif",
"PROCESSOR_SOCKET": "Intel Socket 1155",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1160 million",
"PROCESSOR_DIE_SIZE": "216 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sandy Bridge",
"PROCESSOR_PART": "SR00M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Intel HD 2000",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E7-8870",
"PROCESSOR_SOCKET_IMAGE": "77.gif",
"PROCESSOR_SOCKET": "Intel Socket 1567",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2600 million",
"PROCESSOR_DIE_SIZE": "513 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EX",
"PROCESSOR_PART": "SLC3E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E7-8860",
"PROCESSOR_SOCKET_IMAGE": "77.gif",
"PROCESSOR_SOCKET": "Intel Socket 1567",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2600 million",
"PROCESSOR_DIE_SIZE": "513 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2276 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EX",
"PROCESSOR_PART": "SLC3F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E7-8850",
"PROCESSOR_SOCKET_IMAGE": "77.gif",
"PROCESSOR_SOCKET": "Intel Socket 1567",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "2600 million",
"PROCESSOR_DIE_SIZE": "513 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EX",
"PROCESSOR_PART": "SLC3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Ten-core",
"PROCESSOR_SMPCPUS": "4",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "30720 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3690",
"PROCESSOR_SOCKET_IMAGE": "72.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBW2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5603",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLC2F",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5606",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLC2N",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5607",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBZ9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5647",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBZ7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5672",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBYK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5687",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3866 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5649",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBZ8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5675",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBYL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5690",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5698",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "33.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLC32",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3670",
"PROCESSOR_SOCKET_IMAGE": "72.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBVE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3530",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3066 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBKR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5503",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBKD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5507",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBKC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3680",
"PROCESSOR_SOCKET_IMAGE": "72.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gulftown",
"PROCESSOR_PART": "SLBV2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5620",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2666 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5630",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVB",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5640",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2933 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5667",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5677",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3466 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3733 MHz",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5609",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5618",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2266 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBX3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5630",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBVD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5645",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2666 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBWZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5650",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3066 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5660",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5670",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5638",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBWY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5640",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5680",
"PROCESSOR_SOCKET_IMAGE": "68.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1170 million",
"PROCESSOR_DIE_SIZE": "239 mm²",
"PROCESSOR_PACKAGE": "FC-LGA10",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Westmere-EP",
"PROCESSOR_PART": "SLBV5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "12288 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Celeron P1053",
"PROCESSOR_SOCKET_IMAGE": "133.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "30 W",
"PROCESSOR_CODENAME": "Jasper Forest",
"PROCESSOR_PART": "SLBWN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3565",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3550",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3066 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEY",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3580",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBET",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W5590",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBGE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5530",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2666 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBGF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3520",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2933 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3540",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBEX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3570",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBES",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3503",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.225 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W3505",
"PROCESSOR_SOCKET_IMAGE": "70.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.225 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Bloomfield",
"PROCESSOR_PART": "SLBGC",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5502",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBEZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5504",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF9",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5506",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF8",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5506",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBFH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5508",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "38 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBGK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5520",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2533 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBFD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5530",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2666 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF7",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon E5540",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2533 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF6",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5550",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3066 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF5",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5560",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF4",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon X5570",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2933 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3333 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF3",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon W5580",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3466 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBF2",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5518",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBFW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon L5520",
"PROCESSOR_SOCKET_IMAGE": "71.gif",
"PROCESSOR_SOCKET": "Intel Socket 1366",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "731 million",
"PROCESSOR_DIE_SIZE": "263 mm²",
"PROCESSOR_PACKAGE": "FC-LGA8",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2266 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2533 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Gainestown",
"PROCESSOR_PART": "SLBFA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "256 KB (per core)",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7110M",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7110N",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7120M",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7120N",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7130M",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7130N",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3166 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7140M",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "16384 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 7140N",
"PROCESSOR_SOCKET_IMAGE": "97.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "1328 million",
"PROCESSOR_DIE_SIZE": "435 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "150 W",
"PROCESSOR_CODENAME": "Tulsa",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "16384 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5110",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5120",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1866 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5130",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5140",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5150",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2666 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5160",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5148",
"PROCESSOR_SOCKET_IMAGE": "96.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Woodcrest",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5080",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3730 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL968",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5060",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "130 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL96B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5050",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL96C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5030",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL96E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5040",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2830 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL96D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 5063",
"PROCESSOR_SOCKET_IMAGE": "98.gif",
"PROCESSOR_SOCKET": "Intel Socket 771",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Dempsey",
"PROCESSOR_PART": "SL96B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "DDR2",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "0 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 7041 Dual-Core",
"PROCESSOR_SOCKET_IMAGE": "134.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 7030 Dual-Core",
"PROCESSOR_SOCKET_IMAGE": "125.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 7040 Dual-Core",
"PROCESSOR_SOCKET_IMAGE": "134.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 7030 Dual-Core",
"PROCESSOR_SOCKET_IMAGE": "125.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 7020 Dual-Core",
"PROCESSOR_SOCKET_IMAGE": "134.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 2.8",
"PROCESSOR_SOCKET_IMAGE": "125.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "200 million",
"PROCESSOR_DIE_SIZE": "213 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Paxville",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.33",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.16",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3167 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.33",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.16",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3167 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.00",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "RK80546KF0808M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.00",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "RK80546KF0808M",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 2.83",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 2.83",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.66",
"PROCESSOR_SOCKET_IMAGE": "127.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Cranford",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.50",
"PROCESSOR_SOCKET_IMAGE": "127.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Cranford",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.33",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "4096 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon MP 3.16",
"PROCESSOR_SOCKET_IMAGE": "126.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "286 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3167 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Potomac",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "8192 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 3.6",
"PROCESSOR_SOCKET_IMAGE": "129.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "178 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Irwindale",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 3.4",
"PROCESSOR_SOCKET_IMAGE": "129.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "178 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Irwindale",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 3.2",
"PROCESSOR_SOCKET_IMAGE": "129.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "178 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Irwindale",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
},
{
"PROCESSOR_MODEL_NAME": "Xeon 3.0",
"PROCESSOR_SOCKET_IMAGE": "129.gif",
"PROCESSOR_SOCKET": "Intel Socket 604",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "178 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.412 V",
"PROCESSOR_TDP": "135 W",
"PROCESSOR_CODENAME": "Irwindale",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "16 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "ServerWorkstation"
} 
]}}