{"DATABASE":  [
{
"PROCESSOR_MODEL_NAME": "A10-7850K",
"PROCESSOR_SOCKET_IMAGE": "312.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "28 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kaveri",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon R7",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-7700K",
"PROCESSOR_SOCKET_IMAGE": "312.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "28 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kaveri",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jan 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon R7",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6790K",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "4000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "40.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD679KWOA44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Oct 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8670D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6700T",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD670TYHA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-9370",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4700 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.912 V",
"PROCESSOR_TDP": "220 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD9370FHHKWOF",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-9590",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 5000 MHz",
"PROCESSOR_MULTIPLIER": "23.5x",
"PROCESSOR_VOLTAGE": "1.912 V",
"PROCESSOR_TDP": "220 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD9590FHHKWOF",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6800K",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "4100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4400 MHz",
"PROCESSOR_MULTIPLIER": "41.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD680KWOA44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8670D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-6700",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6700OKA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8670D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-6600K",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "39.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD660KWOA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8570D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-6500",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "35.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6500OKA44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8570D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-6400K",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "39.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD640KOKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8470D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-6300",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "37.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD6300OKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8370D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-4000",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AD4000OKA23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD6350FRW6KHK",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "FC-PGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4350FRW4KHK",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Apr 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 280",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX280OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4130",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4130WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-2000",
"PROCESSOR_SOCKET_IMAGE": "201.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1750 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM2000GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7340",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E1-1500",
"PROCESSOR_SOCKET_IMAGE": "42.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1480 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1500GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8350",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8350FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8300FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8140",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8140WMW8KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8170",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4500 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6120WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6130",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6130WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "19.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4120WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4150",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4150WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD6300WMHKBOX",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4320",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8320",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD8320FRW8KHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4300",
"PROCESSOR_SOCKET_IMAGE": "290.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Vishera",
"PROCESSOR_PART": "FD4300WMW4MHK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5800K",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "38.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD580KWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5600K",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD560KWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5700",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "34.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5700OKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-5400K",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD540KOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7540D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5500",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5500OKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A10-5800B",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "74°C",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "38.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD580BWOA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-5500B",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "32.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD550BOKA44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7560D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-5400B",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3800 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD540BOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7540D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-5300B",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD530BOKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-5300",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FM2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "70°C",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "36.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AD5300OKA23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7480D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E1-1200",
"PROCESSOR_SOCKET_IMAGE": "42.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1200GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-1800",
"PROCESSOR_SOCKET_IMAGE": "201.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EM1800GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7340",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6200",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4100 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6200FRW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4170",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "4200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4300 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4170FRW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 641",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD641XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 638",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD638XOJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3870K",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3870WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3670K",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3670WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3820",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3820OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3620",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3620OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3420",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "28.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3420OJZ22HX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 651",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD651XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 651K",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "30.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD651KWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8150",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4200 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8150FRGUBOX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8120",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 4000 MHz",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8120FRGUBOX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-6100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD6100WMW6KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "288 KB",
"PROCESSOR_CACHEL2": "6144 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-4100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3900 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD4100WMW4KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "FX-8100",
"PROCESSOR_SOCKET_IMAGE": "38.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3+",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1200 million",
"PROCESSOR_DIE_SIZE": "315 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zambezi",
"PROCESSOR_PART": "FD8100WMW8KGU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Eight-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "384 KB",
"PROCESSOR_CACHEL2": "8192 KB",
"PROCESSOR_CACHEL3": "8192 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3400",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3400OJZ22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-3300",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD33000OJZ22HX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6410D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "E2-3200",
"PROCESSOR_SOCKET_IMAGE": "40.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "ED3200OJZ22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6370D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3500",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3500OJZ33GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 631",
"PROCESSOR_SOCKET_IMAGE": "189.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD631XWNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 130",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX130HBK12GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 650T",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD650TWFK4FGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 270",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX270OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3850",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3850WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3650",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "26.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "100 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3650WNZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A6-3600",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3600OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6530D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A8-3800",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FM1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "24.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AD3800OJZ43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6550D",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 850",
"PROCESSOR_SOCKET_IMAGE": "186.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "HDX850WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 980 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ980FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 425e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD425EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 460",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX460WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 620e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD620EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 975 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ975FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 840",
"PROCESSOR_SOCKET_IMAGE": "186.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "HDX840WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1100T BE",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3700 MHz",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDE00ZFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1065T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT65TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 565 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ565WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 455",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX455WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 150",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX150HBK13GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 970 BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HDZ970FBK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 715 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ715WCJ3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1075T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT75TFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 560 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ560WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 210e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD210EHDK22GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 220",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX220OCK22GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 450",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX450WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 970 BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HDZ970FBK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 420e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD420EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 615e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD615EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 645",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX645WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 265",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX265OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 270u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD270USCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR2, DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD250EHDK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 145",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX145HBK13GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1045T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT45TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 840T",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD840TWFK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 180",
"PROCESSOR_SOCKET_IMAGE": "199.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "SDX180HDK22GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 960T BE",
"PROCESSOR_SOCKET_IMAGE": "188.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Zosma",
"PROCESSOR_PART": "HD96ZTWFK4DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 245e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD245EHDK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 260",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX260OCK23GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 415e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD415EHDK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 445",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX445WFK32GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B97",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB97WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B77",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB77WFK3DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B57",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB57WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 610e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD610EHDK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 640",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX640WFK42GM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 570 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ570WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1055T (95W)",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.375 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT55TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1090T BE",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3600 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT90ZFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1055T (125W)",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT55TFBK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X6 1035T",
"PROCESSOR_SOCKET_IMAGE": "31.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "904 million",
"PROCESSOR_DIE_SIZE": "346 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Thuban",
"PROCESSOR_PART": "HDT35TWFK6DGR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Six-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 910e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD910EOCK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 555 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ555WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 255",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX255OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 440",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX440WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 635",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX635WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 720",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDX720WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2010",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 965 BE (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ965FBK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 550",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDX550WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 400e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD400EHDK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 405e",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "AD405EHDK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD250USCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 260u",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.05 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 235e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD235EHDK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 240e",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "AD240EHDK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 215",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX215OCK22GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 425",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX425WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 600e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD600EHDK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 605e",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "AD605EHDK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X3 435",
"PROCESSOR_SOCKET_IMAGE": "36.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Rana",
"PROCESSOR_PART": "ADX435WFK32GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B93",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB93WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 B95",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDXB95WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B73",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB73WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 B75",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDXB75WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B53",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB53WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 B55",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDXB55WFK2DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 620",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX620WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X4 630",
"PROCESSOR_SOCKET_IMAGE": "37.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "300 million",
"PROCESSOR_DIE_SIZE": "169 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Propus",
"PROCESSOR_PART": "ADX630WFK42GI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 740 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ740WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 820",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX820WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 830",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX830WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 965 BE (140W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ965FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 240",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX240OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 245",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX245OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 945 (95W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX945WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 140",
"PROCESSOR_SOCKET_IMAGE": "185.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "234 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sargas",
"PROCESSOR_PART": "SDX140HBK13GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon II X2 250",
"PROCESSOR_SOCKET_IMAGE": "35.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "410 million",
"PROCESSOR_DIE_SIZE": "117 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Regor",
"PROCESSOR_PART": "ADX250OCK23GQ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 700e",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HD700EOCK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 705e",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HD705EOCK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 900e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD900EOCK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 905e",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HD905EOCK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 545",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDX545WFK2DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (per core)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X2 550 BE",
"PROCESSOR_SOCKET_IMAGE": "60.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "80 W",
"PROCESSOR_CODENAME": "Callisto",
"PROCESSOR_PART": "HDZ550WFK2DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II 42 TWKR Black Edition",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 925",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX925WFK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7850 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD785ZWCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 945 (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX945FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ955FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 (125W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX955FBK4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 955 (95W)",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX955WFK4DGM",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 710",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDX710WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 805",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX805WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X3 720 BE",
"PROCESSOR_SOCKET_IMAGE": "20.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Heka",
"PROCESSOR_PART": "HDZ720WFK3DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 810",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX810WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "4096 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 910",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.425 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX910WFK4FGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 920",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDX920XCJ4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom II X4 940 BE",
"PROCESSOR_SOCKET_IMAGE": "21.gif",
"PROCESSOR_SOCKET": "AMD Socket AM3",
"PROCESSOR_PROCESS_SIZE": "45 nm",
"PROCESSOR_TRANSISTORS": "758 million",
"PROCESSOR_DIE_SIZE": "258 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Deneb",
"PROCESSOR_PART": "HDZ940XCJ4DGI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "6144 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2650e",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADG2650IAV4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2009",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7450",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD7450WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7550",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD7550WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 7750 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD775ZWCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 5050e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH5050IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8850",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8850WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9450e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9450ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 (95W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9850WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9950 BE (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD995ZXAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8250e",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8250ODJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8450e",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8450ODJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8750 BE",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD875ZWCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 6500 BE",
"PROCESSOR_SOCKET_IMAGE": "184.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Kuma",
"PROCESSOR_PART": "AD6500WCJ2BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD975BWCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD985BWCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9150e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9150ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9350e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.125 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9350ODJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9850XAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2000+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADF2000IAV4DR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1660",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1660IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600B",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD960BWCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8450",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8450WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8650",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8650WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8750",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8750WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8550",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8550WCJ3BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4050e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4050IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4450e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4450IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADA5800IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1640",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1640IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9100e",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9100OBJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9550",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9550WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9650",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9650WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750 (95W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9750WCJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9750 (125W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9750XAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9850 BE",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD985ZXAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9950 BE (140W)",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "140 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD995ZFAJ4BGH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8400",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8400WCJ3BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X3 8600",
"PROCESSOR_SOCKET_IMAGE": "22.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Toliman",
"PROCESSOR_PART": "HD8600WCJ3BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Triple-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 4850e",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH4850IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2100",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2100IAA4DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2200",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2200IAA4DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2300",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2300IAA4DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron X2 2100",
"PROCESSOR_SOCKET_IMAGE": "183.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "221 million",
"PROCESSOR_DIE_SIZE": "118 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "SDO2100IAA4DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "2",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+ BE",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2600+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.1 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADG2600IAV4DR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600 BE",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD960ZWCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9500",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9500WCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Phenom X4 9600",
"PROCESSOR_SOCKET_IMAGE": "23.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2+",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "450 million",
"PROCESSOR_DIE_SIZE": "285 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "95 W",
"PROCESSOR_CODENAME": "Agena",
"PROCESSOR_PART": "HD9600WCJ4BGD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "2048 KB (shared)",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5200IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2300",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2300IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2350",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2350IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 BE-2400",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADH2400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1250",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1250IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1300",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1300IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1600",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADH1600IAA5DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1620",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADH1620IAA5DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 LE-1640",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH1640IAA4DP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ BE",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6400+ BE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADX6400IAA6CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADV6000IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1100",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1100IAA3DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1150",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1150IAA3DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron LE-1200",
"PROCESSOR_SOCKET_IMAGE": "182.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Sparta",
"PROCESSOR_PART": "SDH1200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+ EE",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADD3500IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 6000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.5x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADV6000IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO5000IAA5CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5400IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO3600IAA5DL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-70",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX70GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-72",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX72GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-74",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX74GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-76",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket F",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "235 mm²",
"PROCESSOR_PACKAGE": "FC-LGA6",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "3200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX76GAA6DI",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3800IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA5200IAA6CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5200IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO5000IAA5CZ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3600+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO3600IAA4CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-62",
"PROCESSOR_SOCKET_IMAGE": "172.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "243 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "125 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADAFX62IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 5000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO5000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4800IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4400IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4000IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4800+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4800IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.075 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADD3800IAT5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4600IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4400+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4400IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4200IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4000+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO4000IAA6CS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+ EE",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADO3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4600IAA5DO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 4200+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO4200IAA5DD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3200IAA2CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3600+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3600IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3200IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+ EE SFF",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDD3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-60",
"PROCESSOR_SOCKET_IMAGE": "176.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "233 million",
"PROCESSOR_DIE_SIZE": "199 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "110 W",
"PROCESSOR_CODENAME": "Toledo",
"PROCESSOR_PART": "ADAFX60DAA6CD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 1500+",
"PROCESSOR_SOCKET_IMAGE": "166.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "0.9 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Venice",
"PROCESSOR_PART": "ADC1500B2X4BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3500+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3500IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3200+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3200IAA2CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3800+",
"PROCESSOR_SOCKET_IMAGE": "171.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "220 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA5CU",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2500+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2500AIO3BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-57",
"PROCESSOR_SOCKET_IMAGE": "178.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "115 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "San Diego",
"PROCESSOR_PART": "ADAFX57DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-55",
"PROCESSOR_SOCKET_IMAGE": "178.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "115 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "San Diego",
"PROCESSOR_PART": "ADAFX55DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-55",
"PROCESSOR_SOCKET_IMAGE": "178.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "115 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "104 W",
"PROCESSOR_CODENAME": "San Diego",
"PROCESSOR_PART": "ADAFX55DAA5BN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2200+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2200DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2400+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2400DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2500+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2500AIO3BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2400+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2400DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2300+",
"PROCESSOR_SOCKET_IMAGE": "192.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1583 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "SDC2300DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2200+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2200DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-53",
"PROCESSOR_SOCKET_IMAGE": "177.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADAFX53DEP5AS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3700+",
"PROCESSOR_SOCKET_IMAGE": "163.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADA3700AEP5AR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3800+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3800IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3700+",
"PROCESSOR_SOCKET_IMAGE": "163.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADA3700AEP5AR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2800+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA2800AEP4AP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2800+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA2800AEP4AP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3300+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3300AEP3AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-53",
"PROCESSOR_SOCKET_IMAGE": "177.gif",
"PROCESSOR_SOCKET": "AMD Socket 939",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADAFX53DEP5AS",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 3100+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL3100DKV3E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 FX-51",
"PROCESSOR_SOCKET_IMAGE": "169.gif",
"PROCESSOR_SOCKET": "AMD Socket 940",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "SledgeHammer",
"PROCESSOR_PART": "ADAFX51CEP5AK",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2400+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2400DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2400+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2400DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2200+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2200DUV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2000+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2000DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2200+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2200DUV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2000+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2000DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL2600DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL2600DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2500+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDA2500DKV4D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2500+ DTR",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1833 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDL2500DLV4D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2700+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2167 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA2700DKV3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL2600DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2800+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2250 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "74 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA2800DKV3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL2600DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2400+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2400DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2400+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2400DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2200+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2200DUV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2000+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2000DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2000+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2000DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1800+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "51 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA1800DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2100+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "72 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX2100DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2000+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2000DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1900+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1900DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1800+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "51 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA1800DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1700+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1467 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "64 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1700DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1600+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1600DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1500+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1500DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1400",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "72 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1400AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2001",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1400",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "72 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1400AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2001",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1333",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1333 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "70 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1333AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2001",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1300",
"PROCESSOR_SOCKET_IMAGE": "241.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thunderbird B",
"PROCESSOR_PART": "A1300AMS3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2001",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2500+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2500AIO3BX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2400+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1667 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2400DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2300+",
"PROCESSOR_SOCKET_IMAGE": "192.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1583 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "SDC2300DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jul 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2200+",
"PROCESSOR_SOCKET_IMAGE": "193.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "SDC2200DUT3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 3200+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "77 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDA3200DKV4E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 3000+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDA3000DKV4E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 3000+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDA3000DKV4E",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2800+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2250 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "74 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA2800DKV3D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDL2600DKV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2800+ DTR",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2083 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDL2800DLV4D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2600+ DTR",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1917 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXDL2600DLV4D",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2200+",
"PROCESSOR_SOCKET_IMAGE": "190.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Thorton",
"PROCESSOR_PART": "AXDC2200DUV3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2003",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 2100+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1733 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "72 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX2100DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1900+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "68 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1900DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1800+",
"PROCESSOR_SOCKET_IMAGE": "233.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "80 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.6 V",
"PROCESSOR_TDP": "51 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXDA1800DUT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1700+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1467 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "64 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1700DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1700+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1467 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "64 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1700DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP 1600+",
"PROCESSOR_SOCKET_IMAGE": "196.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "150 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Palomino",
"PROCESSOR_PART": "AX1600DMT3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 X2 3600+",
"PROCESSOR_SOCKET_IMAGE": "4.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "126 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.25 V",
"PROCESSOR_TDP": "65 W",
"PROCESSOR_CODENAME": "Brisbane",
"PROCESSOR_PART": "ADO3600IAA5DL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3500+",
"PROCESSOR_SOCKET_IMAGE": "174.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "227 million",
"PROCESSOR_DIE_SIZE": "230 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Windsor",
"PROCESSOR_PART": "ADA3500IAA4DH",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3700+",
"PROCESSOR_SOCKET_IMAGE": "163.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADA3700AEP5AR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1200",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "66 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1200AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1133",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1133 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "63 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1133AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1000",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1000AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1200",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "66 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1200AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1100",
"PROCESSOR_SOCKET_IMAGE": "241.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "60 W",
"PROCESSOR_CODENAME": "Thunderbird B",
"PROCESSOR_PART": "A1100AMS3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 1000",
"PROCESSOR_SOCKET_IMAGE": "237.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "54 W",
"PROCESSOR_CODENAME": "Thunderbird C",
"PROCESSOR_PART": "A1000AMS3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 950",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "950 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "52 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0950AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 900",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "50 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0900AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 850",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "850 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "47 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0850AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 800",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0800AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 750",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "750 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "43 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0750AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 600",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "38 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0600AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 700",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "700 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "7.0x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "40 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0700AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 650",
"PROCESSOR_SOCKET_IMAGE": "242.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "180 nm",
"PROCESSOR_TRANSISTORS": "37 million",
"PROCESSOR_DIE_SIZE": "120 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "650 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "6.5x",
"PROCESSOR_VOLTAGE": "1.75 V",
"PROCESSOR_TDP": "38 W",
"PROCESSOR_CODENAME": "Thunderbird",
"PROCESSOR_PART": "A0650AMT3B",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2000",
"PROCESSOR_MEMORYSUPPORT": "DDR1",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "A4-5050",
"PROCESSOR_SOCKET_IMAGE": "304.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Feb 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8330",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E1-2150",
"PROCESSOR_SOCKET_IMAGE": "302.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1050 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Feb 2014",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-1350",
"PROCESSOR_SOCKET_IMAGE": "304.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Oct 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5750M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5750DEC44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5550M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5550DEC44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8550G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5350M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5350DEC23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8450G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5150M",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "105°C",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3300 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5150DEC23HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8350G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5557M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3100 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5557DFE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8550G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5745M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2900 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5745SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8610G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-5757M",
"PROCESSOR_SOCKET_IMAGE": "301.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5757DFE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8650G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-5545M",
"PROCESSOR_SOCKET_IMAGE": "300.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5545SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8510G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5145M",
"PROCESSOR_SOCKET_IMAGE": "298.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5145SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8310G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5345M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5345SIE44HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8410G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5357M",
"PROCESSOR_SOCKET_IMAGE": "299.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "71°C",
"PROCESSOR_FREQUENCY": "2900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3500 MHz",
"PROCESSOR_MULTIPLIER": "29.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Richland",
"PROCESSOR_PART": "AM5357DFE23HL",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "Jun 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8450G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-1450",
"PROCESSOR_SOCKET_IMAGE": "297.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1400 MHz",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1450IDJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8250",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-1250",
"PROCESSOR_SOCKET_IMAGE": "296.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "8 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1250IDJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-1200",
"PROCESSOR_SOCKET_IMAGE": "296.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "4 W",
"PROCESSOR_CODENAME": "Temash",
"PROCESSOR_PART": "AT1200IFJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8180",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E1-2100",
"PROCESSOR_SOCKET_IMAGE": "302.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM2100ICJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8210",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E1-2500",
"PROCESSOR_SOCKET_IMAGE": "302.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM2500IBJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8240",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E2-3000",
"PROCESSOR_SOCKET_IMAGE": "303.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1650 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "EM3000IBJ23HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8280",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-5000",
"PROCESSOR_SOCKET_IMAGE": "304.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "15 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "AM5000IBJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8330",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-5200",
"PROCESSOR_SOCKET_IMAGE": "305.gif",
"PROCESSOR_SOCKET": "AMD Socket FT3",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "90°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.475 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Kabini",
"PROCESSOR_PART": "AM5200IAJ44HM",
"PROCESSOR_PRODUCTION_STATUS": "Active",
"PROCESSOR_RELEASED": "May 2013",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 8400",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Z-60",
"PROCESSOR_SOCKET_IMAGE": "235.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "5 W",
"PROCESSOR_CODENAME": "Hondo",
"PROCESSOR_PART": "XMZ60AFVB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-4355M",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1303 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4355SHE23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7400G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-4555M",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "19 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4555SHE44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7600G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-70",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1333 MHz",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC70AFPB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6290",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-4600M",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "23.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4600DEC44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7660G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-4500M",
"PROCESSOR_SOCKET_IMAGE": "45.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.3 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4500DEC44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7640G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-4400M",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3200 MHz",
"PROCESSOR_MULTIPLIER": "27.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4400DEC23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7520G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A10-4655M",
"PROCESSOR_SOCKET_IMAGE": "39.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2800 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4655SIE44HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7620G",
"PROCESSOR_CACHEL1": "192 KB",
"PROCESSOR_CACHEL2": "4096 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-4455M",
"PROCESSOR_SOCKET_IMAGE": "46.gif",
"PROCESSOR_SOCKET": "AMD Socket FP2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "BGA2",
"PROCESSOR_TCASEMAX": "100°C",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.15 V",
"PROCESSOR_TDP": "17 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4455SHE24HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7500G",
"PROCESSOR_CACHEL1": "92 KB",
"PROCESSOR_CACHEL2": "2048 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-4300M",
"PROCESSOR_SOCKET_IMAGE": "43.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1r2",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1303 million",
"PROCESSOR_DIE_SIZE": "246 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 3000 MHz",
"PROCESSOR_MULTIPLIER": "25.0x",
"PROCESSOR_VOLTAGE": "1.325 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Trinity",
"PROCESSOR_PART": "AM4300DEC23HJ",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2012",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 7420G",
"PROCESSOR_CACHEL1": "96 KB",
"PROCESSOR_CACHEL2": "1024 KB (shared)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E2-3000M",
"PROCESSOR_SOCKET_IMAGE": "40.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "EM3000DDX22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6380G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3320M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3320DDX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3330MX",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "22.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3330HLX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3420M",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3420DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3430MX",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1700 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "17.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3430HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3520M",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3520DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3550MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2700 MHz",
"PROCESSOR_MULTIPLIER": "20.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3550HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-450",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1650 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME450GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6320",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-300",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME300GBB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-60",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "up to 1333 MHz",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC60AFPB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6290",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3300M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3300DDX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3305M",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3305DDX22GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A4-3310MX",
"PROCESSOR_SOCKET_IMAGE": "33.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "21.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3310HLX23GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6480G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3400M",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1400 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3400DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A6-3410MX",
"PROCESSOR_SOCKET_IMAGE": "34.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2300 MHz",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3410HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6520G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3500M",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2400 MHz",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3500DDX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3510MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2500 MHz",
"PROCESSOR_MULTIPLIER": "18.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3510HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "A8-3530MX",
"PROCESSOR_SOCKET_IMAGE": "32.gif",
"PROCESSOR_SOCKET": "AMD Socket FS1",
"PROCESSOR_PROCESS_SIZE": "32 nm",
"PROCESSOR_TRANSISTORS": "1178 million",
"PROCESSOR_DIE_SIZE": "228 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "up to 2600 MHz",
"PROCESSOR_MULTIPLIER": "19.0x",
"PROCESSOR_VOLTAGE": "1.4125 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Llano",
"PROCESSOR_PART": "AM3530HLX43GX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "DDR3",
"PROCESSOR_OFCORES": "Quad-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6620G",
"PROCESSOR_CACHEL1": "128 KB (per core)",
"PROCESSOR_CACHEL2": "1024 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Z-01",
"PROCESSOR_SOCKET_IMAGE": "234.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "5.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "6 W",
"PROCESSOR_CODENAME": "Desna",
"PROCESSOR_PART": "XMZ01AFVB22GV",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-350",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME350GBB22GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "E-240",
"PROCESSOR_SOCKET_IMAGE": "57.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "18 W",
"PROCESSOR_CODENAME": "Zacate",
"PROCESSOR_PART": "EME240GBB12GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6310",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-30",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC30AFPB12GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "C-50",
"PROCESSOR_SOCKET_IMAGE": "41.gif",
"PROCESSOR_SOCKET": "AMD Socket FT1",
"PROCESSOR_PROCESS_SIZE": "40 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "75 mm²",
"PROCESSOR_PACKAGE": "",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "9 W",
"PROCESSOR_CODENAME": "Ontario",
"PROCESSOR_PART": "CMC50AFPB22GT",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2011",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "Radeon HD 6250",
"PROCESSOR_CACHEL1": "64 KB (per core)",
"PROCESSOR_CACHEL2": "512 KB (per core)",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-74",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM74DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-75",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM75DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-77",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM77DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-88",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2500 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-64",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL64DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-65",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL65DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-67",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL67DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Dec 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-72",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM72DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-84",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM84DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-85",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2300 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM85DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-62",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL62DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Sep 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-80",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2100 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "32 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM80DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-82",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM82DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-86",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMZM86DAM23GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 Ultra ZM-87",
"PROCESSOR_SOCKET_IMAGE": "59.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "2048 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon X2 QL-60",
"PROCESSOR_SOCKET_IMAGE": "6.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1900 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.5x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "AMQL60DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2008",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion X2 RM-70",
"PROCESSOR_SOCKET_IMAGE": "25.gif",
"PROCESSOR_SOCKET": "AMD Socket S1",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "unknown",
"PROCESSOR_DIE_SIZE": "unknown",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "unknown",
"PROCESSOR_TDP": "31 W",
"PROCESSOR_CODENAME": "Griffin",
"PROCESSOR_PART": "TMRM70DAM22GG",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Dual-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "256 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3600+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3600IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3400+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3400IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-44",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML44BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-42",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML42BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Oct 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 4000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA4000IAA4CW",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-40",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT40BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-37",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT37BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3300+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3300AIO2BO",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-40",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML40BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-28",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "32 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML28BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-28",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "22 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT28BQX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3400+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA3400AEP4AX",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3700+",
"PROCESSOR_SOCKET_IMAGE": "163.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "105 million",
"PROCESSOR_DIE_SIZE": "193 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2400 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "12.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "Clawhammer",
"PROCESSOR_PART": "ADA3700AEP5AR",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jun 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3200+",
"PROCESSOR_SOCKET_IMAGE": "175.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "65 nm",
"PROCESSOR_TRANSISTORS": "122 million",
"PROCESSOR_DIE_SIZE": "77 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Lima",
"PROCESSOR_PART": "ADH3200IAA4DE",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Feb 2007",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-37",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "10.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML37BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-34",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML34BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-34",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMSMT34BQX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-32",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML32BKX4LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-32",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "25 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 ML-30",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "35 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "TMDML30BKX5LD",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Turion 64 MT-30",
"PROCESSOR_SOCKET_IMAGE": "24.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "114 million",
"PROCESSOR_DIE_SIZE": "125 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "22 W",
"PROCESSOR_CODENAME": "Lancaster",
"PROCESSOR_PART": "",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Mar 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "1024 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 3000+",
"PROCESSOR_SOCKET_IMAGE": "170.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "154 million",
"PROCESSOR_DIE_SIZE": "183 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Orleans",
"PROCESSOR_PART": "ADA3000IAA4CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2800+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.5 V",
"PROCESSOR_TDP": "89 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "ADA2800AEP4AP",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon 64 2700+",
"PROCESSOR_SOCKET_IMAGE": "162.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "69 million",
"PROCESSOR_DIE_SIZE": "144 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.2 V",
"PROCESSOR_TDP": "32 W",
"PROCESSOR_CODENAME": "NewCastle",
"PROCESSOR_PART": "unknown",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2200+",
"PROCESSOR_SOCKET_IMAGE": "7.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXMH2200FQQ3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2800+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA2800IAA2CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 2600+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA2600AIO2BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Aug 2004",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "128 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 3000+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2200 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "16.5x",
"PROCESSOR_VOLTAGE": "1.65 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXMA3000FKT4C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2600+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "2000 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "15.0x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXMG2600FQQ4C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2500+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1862 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "14.0x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXMH2500FQQ4C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2400+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXMH2400FQQ4C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2200+",
"PROCESSOR_SOCKET_IMAGE": "7.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "13.5x",
"PROCESSOR_VOLTAGE": "1.45 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Thoroughbred",
"PROCESSOR_PART": "AXMH2200FQQ3C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Nov 2002",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Athlon XP-M 2000+",
"PROCESSOR_SOCKET_IMAGE": "191.gif",
"PROCESSOR_SOCKET": "AMD Socket A",
"PROCESSOR_PROCESS_SIZE": "130 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "101 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1533 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "11.5x",
"PROCESSOR_VOLTAGE": "1.35 V",
"PROCESSOR_TDP": "45 W",
"PROCESSOR_CODENAME": "Barton",
"PROCESSOR_PART": "AXMD2000GJQ4C",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Jan 2001",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "512 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Mobile"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3000+",
"PROCESSOR_SOCKET_IMAGE": "181.gif",
"PROCESSOR_SOCKET": "AMD Socket AM2",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "81 million",
"PROCESSOR_DIE_SIZE": "103 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1600 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "8.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Manila",
"PROCESSOR_PART": "SDA3000IAA3CN",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "May 2006",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
},
{
"PROCESSOR_MODEL_NAME": "Sempron 3100+",
"PROCESSOR_SOCKET_IMAGE": "180.gif",
"PROCESSOR_SOCKET": "AMD Socket 754",
"PROCESSOR_PROCESS_SIZE": "90 nm",
"PROCESSOR_TRANSISTORS": "63 million",
"PROCESSOR_DIE_SIZE": "84 mm²",
"PROCESSOR_PACKAGE": "uPGA",
"PROCESSOR_TCASEMAX": "unknown",
"PROCESSOR_FREQUENCY": "1800 MHz",
"PROCESSOR_TURBOCLOCK": "NA",
"PROCESSOR_MULTIPLIER": "9.0x",
"PROCESSOR_VOLTAGE": "1.4 V",
"PROCESSOR_TDP": "62 W",
"PROCESSOR_CODENAME": "Palermo",
"PROCESSOR_PART": "SDA3100AIO3BA",
"PROCESSOR_PRODUCTION_STATUS": "unknown",
"PROCESSOR_RELEASED": "Apr 2005",
"PROCESSOR_MEMORYSUPPORT": "unknown",
"PROCESSOR_OFCORES": "Single-core",
"PROCESSOR_SMPCPUS": "1",
"PROCESSOR_INTEGRATEDGRAPHIC": "NA",
"PROCESSOR_CACHEL1": "128 KB",
"PROCESSOR_CACHEL2": "256 KB",
"PROCESSOR_CACHEL3": "0 KB",
"PROCESSOR_MARKET": "Desktop"
}
]}}
