i-nex-dimms(1)

NAME
i-nex-dimms - decode the information found in memory module SPD EEPROMs

SYNOPSIS
i-nex-dimms [-c] [-f [-b]] [-x|-X file [files..]]
i-nex-dimms -h

DESCRIPTION
The purpose of the i-nex-dimms tool is to decode the information found in memory module SPD EEPROMs. The SPD data is read either from the running system or dump files. In the former case, the tool requires either the eeprom kernel module or the at24 kernel module to be loaded.

PARAMETERS

-f, --format
    Print nice html output

-b, --bodyonly
    Don't print html header (useful for postprocessing the output)

--side-by-side
    Display all DIMMs side-by-side if possible

--merge-cells
    Merge neighbour cells with identical values (side-by-side output only, default)

--no-merge-cells
    Don't merge neighbour cells with identical values (side-by-side output only)

-c, --checksum
    Decode completely even if checksum fails

-x  Read data from hexdump files

-X  Same as -x except treat multibyte hex data as little endian

-h, --help
    Display the usage summary

SEE ALSO
decode-vaio(1)

AUTHORS
Philip Edelbrock, Christian Zuckschwerdt, Burkart Lingner, Jean Delvare